
               RAYON  PCIPort Adapter  DOCUMENTATION FOR WIN95/98/Me
               -----------------------------------------------------

   DRIVER INSTALLATION

      If you currently have an driver installed, please remove it .After
      removing the driver, reboot your system.  This is necessary because
      P&P will not allow a new driver to be installed until the driver
      is unloaded from memory.

        Once Windows 95 has started, the PLUG & PLAY function of 95 system
      will find the new PCIPORT card. If this is the first time to install
      PCIPORT card in your 95 system. You will be informed to install the
      driver. Just put our PCIPORT driver diskette to driver. Please follow
      the instruction to input the COM port number start value for first
      card and second card.

        Because the resource will be assigned by PCI BIOS. It is not easy
      to check the first card or sencond card by resource. So we have one
      jumper to set this card to be first one or second one. Then we can
      fix the COM port number for each card. (Traditionly, user can not
      confirm the COM port number for each card. Because it will depend
      the card numbers in one system, card slot number and the installation
      sequence. So you may have wrong COM port number for different
      condition and time point.)

        After you had installed PCIPORT driver in one 95 system. You will
      be informed to have new hardware found. But 95 system will install
      the COM port automatically.


Note for multi-P588/P584 card installation.

 1. We can install upto two PCIPORT cards in one 95 system.

 2. When we need to install two PCIPORT cards in one 95 system, we must
    let one card to have jumper ON and the other card to have jumper OFF.

 3. The card with jumper ON is the first card. The card with
    jumper OFF is the second card. We can specify the start COM port number
    for first card and second card seperately.

 4. If user install P588 and P584 card in one 95 system simultaneously,
    please confirm that the COM port number do not overlap. Or you may have
    only one COM port to be actived. Of course this condition must be
    confirmed with other COM port card in the same 95 system.

 5. P584/P588 card can be used in interrupt shared mode. PCI BIOS will
    assign the interrupt for each P588/P584 card. For multi-P584/P588 card
    we can have same IRQ. But user must confirm that one system have
    one IRQ or more to be assigned in P588/P584 card. If there are no IRQ
    left to be assigned for P588/P584 card, we may have wrong process in
    P588/P584 function.
